Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-12-14
P. 38

    UF4E13E0.book  Page 33  Friday, April 27, 2018  2:35 PM

                            Control function operation

                            LOCK” indicator light blinks  two or  three  Insert the clip  under  the engine  shut-off
                            times, then comes on. This indicates the un-  switch before starting the engine.
                            lock mode is selected.
                                                                                         1
                                      1  L-Mode            2
                                                                                                   2

                                                                                                 3

                                                                   1 Engine shut-off switch
                              1 “L-Mode” (unlock) button           2 Clip
                              2 “UNLOCK” indicator light           3 Engine shut-off cord (lanyard)
                            EJU31153                              When the engine is not running, remove the
                            Engine stop switch “ ”
                                                                  clip from the engine shut-off switch to pre-
                            The engine stop switch (red button) stops the
                                                                  vent accidental starting or unauthorized op-
                            engine when the switch is pushed.
                                                                  eration by children or others.

                                                 1

                              1 Engine stop switch
                                                                  EJU42323
                            EJU31164                              Start switch “  ”
                            Engine shut-off switch “  ”
                                                                  ECJ01311
                            The  engine shut-off switch  automatically  NOTICE
                            stops the engine when the clip, on the end of
                                                                  Do not run the engine over 4000 r/min on
                            the engine shut-off cord (lanyard), is removed
                                                                  land. Also, do not run the engine for more
                            from the switch, such as if the operator falls
                                                                  than 15 seconds without supplying water,
                            off the watercraft.
                                                                  otherwise the engine could overheat.
                                                                  The start switch (green button) starts the en-
                                                                  gine when the switch is pushed.
                                                                  Release the start switch as soon as the en-
                                                                  gine starts to run. If the engine does not start

                            33

| 33 34 35 36 37 38 39 40 41 42 43 |