Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-14
P. 52

    UF4E13E0.book  Page 47  Friday, April 27, 2018  2:35 PM

                            Instrument operation

                            warning is activated, the  maximum  engine  If the engine is stopped after the check en-
                            speed is limited.                     gine warning is activated, the information dis-
                                                                  play will indicate an error code.

                            If the engine overheat warning is activated,
                            immediately reduce the engine speed, return  If the check engine warning is activated, im-
                            to shore, and then make sure that water is  mediately reduce the engine speed, return to
                            being discharged from the cooling water pilot  shore, and have a Yamaha dealer check the
                            outlet while the engine is running. If there is  engine.
                            no discharge of water, stop the engine, and  EJU43740
                                                                  Hour meter
                            then check the jet intake for clogging. (See
                                                                  The hour meter shows the total number of
                            page 99 for information  on the  jet intake.)
                                                                  hours that the engine has been running since
                            NOTICE: If you cannot locate and correct
                                                                  the watercraft was new.
                            the  cause of the  overheating, consult  a
                            Yamaha dealer. Continuing to operate at  TIP:
                            higher speeds could result in severe en-  The elapsed time will be kept even if the bat-
                                                                  tery terminals have been disconnected.
                            gine damage. [ECJ00042]

                                                                                 1
                                                                   1 Hour meter
                            EJU43731
                            Check engine warning                  EJU43751
                            If a sensor malfunction or a short circuit is de-  Voltmeter
                            tected, the check engine  warning  indicator  The voltmeter shows the battery voltage.
                            and the “WARNING” indicator light blink, and  When the battery voltage is normal, the volt-
                            the buzzer sounds intermittently for 30 sec-  meter displays approximately 12 volts.
                            onds.

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |