Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-12-14
P. 70

    UF4E13E0.book  Page 65  Friday, April 27, 2018  2:35 PM

                            Pre-operation checks

                            EJU32282                              Make sure that there is no damage inside the
                               Pre-operation check points
                                                                  engine compartment.
                            EJU42383
                            Pre-launch checks
                            Perform the pre-launch checks in the pre-op-
                            eration checklist while the watercraft is  on
                            land.
                            To perform the pre-launch checks:
                            (1) Remove the seats and removable water-
                                tight storage compartment. (See page 49
                                for seat removal and installation proce-
                                dures and page 54 for information on the
                                removable watertight storage compart-
                                ment.)                            EJU34215
                                                                  Fuel system checks
                            (2) Perform the checks and make sure that  EWJ00382
                                there are no malfunctioning items or oth-  WARNING
                                er problems.                      Leaking fuel can result in fire or explosion.
                            (3) After completing these checks, securely   Check for fuel leakage regularly.
                                install the removable watertight storage   If any fuel leakage is found, the fuel sys-
                                compartment and seats in their original  tem must be repaired by a qualified me-
                                positions.                         chanic. Improper repairs can make the
                            EJU32334
                            Engine compartment check               watercraft unsafe to operate.
                            EWJ00462
                                 WARNING                          Make sure that there is no damage, leakage,
                                                                  or other problem in the fuel system.
                            Failure  to  ventilate the engine compart-
                                                                  Check:
                            ment could result in a fire or explosion. Do
                                                                   Fuel filler cap and seal for damage
                            not start the engine if there is a fuel leak.
                                                                   Fuel tank for damage and leakage
                            Ventilate the engine compartment. Leave the   Fuel hoses and joints for damage and leak-
                            engine compartment open for a few minutes  age
                            to allow any fuel vapors to escape.    Fuel tank breather hose  for damage and
                                                                   leakage
                                                                  EJU36875
                                                                  Fuel level check
                                                                  Check the fuel level in the fuel tank.
                                                                  Add fuel if necessary. (See page 56 for infor-
                                                                  mation on filling the fuel tank.)

                            65

| 65 66 67 68 69 70 71 72 73 74 75 |