Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-12-14
P. 85

    UF4E13E0.book  Page 80  Friday, April 27, 2018  2:35 PM

                                                                                      Operation

                            (2) Pull yourself up to a kneeling position on  holding on to the person in front of them
                                the boarding platform, and then move to  or to the handgrip provided.
                                the seat and sit astride.          Before boarding the watercraft, make
                                                                   sure that  the engine is  stopped. If the
                                                                   engine is running, the reverse gate may
                                                                   move  down  and a person boarding
                                                                   could be pinched.

                                                                  The heavier the total weight of the operator
                                                                  and passenger(s), the more difficult it will be
                                                                  to balance the watercraft. Do not operate the
                                                                  watercraft when the total weight exceeds 240
                                                                  kg (530 lb) including any cargo.
                                                                  To board with passenger(s):
                            (3) Attach the engine shut-off cord (lanyard)
                                                                  (1) Board as noted in the previous section
                                to your left wrist, and then attach the clip
                                                                     “Boarding alone”.
                                to the engine shut-off switch.
                            (4) Grip the handlebars with both hands and
                                place both feet on the floor of the foot-
                                well.

                                                                  (2) Grip the handlebars with both hands and
                                                                     place both feet on the floor of the foot-
                                                                     well.
                                                                  (3) Have the first passenger move to the rear
                            (5) Look in  all  directions, start the engine,
                                                                     of the watercraft.
                                and then start off slowly.
                            EJU43260
                            Boarding with passenger(s)
                            EWJ01800
                                 WARNING
                             Severe internal injuries can occur if wa-
                              ter is forced into body cavities as a re-
                              sult of being near the jet thrust nozzle.
                              Do not start the engine until the passen-
                              gers are  seated  with their feet on the
                              floor of the footwell and are securely

                                                                                                   80

| 80 81 82 83 84 85 86 87 88 89 90 |