Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-14
P. 48

    UF4E13E0.book  Page 43  Friday, April 27, 2018  2:35 PM

                            Watercraft operation

                            and the engine will respond normally to the  sound one time quickly and the set engine
                            throttle operation.                   speed will change. However, the adjustment
                                                                  is limited to a maximum of five increments
                                                                  above or below the initial cruise assist set-
                                                                  ting.
                                                       1
                                                                  To deactivate the cruise assist:
                                                       2          Relax your grip on the throttle lever. The
                                                                  beeper sounds two times quickly and the dig-
                                                                  ital speedometer display stops blinking when
                                                                  the cruise assist is deactivated.
                                                       3

                              1 Cruise assist up switch
                              2 Cruise assist down switch
                              3 “SET” switch

                            TIP:
                            Once the  cruise  assist is activated, the  set
                            engine speed can be increased by pushing
                            the cruise assist up switch or decreased by
                            pushing the cruise assist down switch. Each
                            time  a switch  is pushed, the  beeper will

                            43

| 43 44 45 46 47 48 49 50 51 52 53 |