Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-15
P. 50

    UF4G13E0.book  Page 45  Friday, April 27, 2018  3:10 PM

                            Instrument operation

                            By switching the display units, the speed can  The outer numbers × 1000 r/min and display
                            be shown in kilometers per hour “km/h” or  segments on the meter show the engine
                            miles per hour “MPH”.                 speed.
                            TIP:
                            “MPH” is selected as the display unit at the
                            Yamaha factory.
                            To switch the speedometer display units:
                            Start the engine, stop the engine, and then
                            push the engine stop switch 3 times, pushing
                            the switch for 0.4 seconds or more each time,
                            before the  multifunction information center
                            turns  off. The speedometer display  units    1
                            change.
                                                                   1 Tachometer
                            To  switch the speedometer display units
                                                                  EJU43891
                            again, repeat this procedure.         Shift indicator (VX / VX Deluxe /
                                                                  VX Cruiser / VX Limited)
                                                                  This indicator shows the  reverse  gate shift
                                                                  positions: “F” (forward), “N” (neutral), and “R”
                                                                  (reverse).  (See page 37 for shifting proce-
                                                                  dures.)

                                                 1
                                                                                                  2
                              1 Engine stop switch
                                                                                                  3

                                                                                                  4
                                                                                   1
                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU31515
                                                                  Fuel level meter
                                               1
                                                                  The fuel level meter shows the amount of fuel
                              1 Speedometer
                                                                  remaining in the fuel tank. The amount of re-
                            EJU31464                              maining fuel  is  shown using eight display
                            Tachometer
                            The tachometer shows the engine speed.  segments, which disappear two at a time as
                                                                  the fuel level decreases.

                            45

| 45 46 47 48 49 50 51 52 53 54 55 |