Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 96 - LIT-18626-12-15
P. 96

    UF4G13E0.book  Page 91  Friday, April 27, 2018  3:10 PM

                            Care and storage

                                case cover. NOTICE: Do not lift up the  (5) Make sure that the area around the wa-
                                air filter case cover forcefully. Other-  tercraft is clear, and then start the engine
                                wise, the fuel hose that is secured to  in a well-ventilated area and let it run at
                                the air filter case cover could be dam-  idle for 15 seconds. (See page 33 for in-
                                aged. [ECJ02620]                     formation on starting the engine.)
                                                                  (6) Stop the engine.
                                                                  (7) Securely install the seats in their original
                                                                     positions.
                                2

                                 1
                              1 Hook
                              2 Air filter case cover
                            (3) Spray a rust inhibitor such as Yamalube
                                Stor-Rite Engine Fogging Oil into the in-
                                take opening for 3 seconds. WARNING!
                                Do not spray flammable rust inhibitor
                                products on engine surfaces while the
                                engine is hot. The sprayed substance
                                or propellants could catch fire. [EWJ00262]

                                               1

                              1 Intake opening
                            (4) Place the air filter case cover in its origi-
                                nal position, and then fit the hooks onto
                                the cover.
                            TIP:
                            Make sure that the air filter case cover is se-
                            curely installed.

                            91

| 91 92 93 94 95 96 97 98 99 100 101 |