Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 84 - LIT-18626-12-15
P. 84

    UF4G13E0.book  Page 79  Friday, April 27, 2018  3:10 PM

                            Operation

                            EJU43445                              current location. (See page 37 for shift sys-
                            Operating the watercraft in reverse or
                                                                  tem operation procedures.)
                            neutral (VX / VX Deluxe / VX Cruiser /
                            VX Limited)
                            Operating in reverse
                            When the RiDE lever is squeezed, the “R” (re-
                            verse) shift indicator will be displayed and the
                            watercraft will move in reverse. (See page 37
                            for shift system operation procedures.)

                                                                                   1
                                                                   1 “N” (Neutral position)

                                             1
                              1 “R” (Reverse position)

                                                                  EJU36087
                                                                  Boarding the watercraft
                                                                  EWJ01112
                                                                      WARNING
                                                                  Be sure the operator and any passengers
                                                                  have practiced boarding from the water
                                                                  while still close to shore before riding. A
                            Make sure that there are no obstacles or peo-  person who has made many unsuccessful
                            ple behind you before shifting into reverse.  attempts to get back on the watercraft
                            TIP:                                  may become fatigued and suffer from ex-
                            This model is equipped with a function which  posure, increasing the  risk of injury and
                            limits the engine speed in reverse.   drowning.
                            Operating in neutral                  Board the watercraft in water free from
                            When the RiDE lever is squeezed lightly and
                                                                  weeds and debris and at least 60 cm (2 ft)
                            released, the “N” (neutral) shift indicator will
                                                                  deep  from the bottom of  the watercraft.
                            be displayed and the watercraft will stop in its
                                                                  NOTICE: Never run the engine in water
                                                                  that is less than 60 cm (2 ft) deep from the
                                                                  bottom of the watercraft, otherwise peb-

                            79

| 79 80 81 82 83 84 85 86 87 88 89 |