Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-12-15
P. 83

    UF4G13E0.book  Page 78  Friday, April 27, 2018  3:10 PM

                                                                                      Operation

                                tercraft will turn gradually while slowing  proximately 100 m (330 ft) after the throttle le-
                                down.                             ver is released or the engine is  stopped,
                                                                  although this distance will vary depending on
                                                                  many factors, including gross weight, water
                                                                  surface conditions, and wind direction.
                               E

                                                            1

                              1 Reverse gate
                            This model is equipped with the Yamaha En-
                            gine Management  System (YEMS) that  in-
                            cludes an off-throttle steering (OTS) system.  VX / VX Deluxe / VX Cruiser / VX Limited: If
                            It will activate at planing speeds should you  the RiDE lever is squeezed to slow down, the
                            attempt to steer the watercraft after releasing  stopping distance is approximately 30%
                            the throttle lever (see condition C above).  shorter than when the RiDE lever is not used.
                            The OTS system assists in turning by con-  However,  this distance will  vary depending
                            tinuing to supply some thrust while the water-  on many factors, including gross weight, wa-
                            craft is decelerating, but you can turn more  ter surface conditions, and wind direction.
                            sharply if you apply throttle while turning the  EWJ01792
                            handlebars. The OTS system does not func-  WARNING
                            tion below planing speeds or when the en-   Allow adequate stopping distance.
                            gine is off. Once the engine slows down, the   Take early action to avoid collisions. Re-
                            watercraft will no longer turn in response to  member, watercraft and other boats do
                            handlebar input until you apply throttle again  not have brakes.
                            or you reach trolling speed.           Operate defensively at safe speeds and
                            EJU45000                               keep a safe distance away from people,
                            Stopping the watercraft                objects, and other watercraft to give you
                            The watercraft is not equipped with a sepa-
                                                                   time to stop.
                            rate braking system.  The watercraft slows
                                                                   Do not shut the engine off when slowing
                            down by water resistance or, when operating
                                                                   down in case you need engine power to
                            in reverse, by the water jet. The watercraft
                                                                   steer away from a boat or other obstacle
                            slows down as soon as the throttle lever is re-
                                                                   that comes into your path.
                            leased, but will coast for a distance before
                                                                   VX / VX Deluxe / VX Cruiser / VX Limited:
                            fully stopping.  If you  are not  sure you  can
                                                                   To avoid rear-end collisions while oper-
                            stop in time before hitting an obstacle, apply
                                                                   ating the watercraft, check behind you
                            throttle and turn in another direction.
                                                                   before using the RiDE lever to slow down
                            From full speed, the watercraft comes to a
                                                                   or stop the watercraft.
                            complete stop due to water resistance in ap-
                                                                                                   78

| 78 79 80 81 82 83 84 85 86 87 88 |