Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-12-15
P. 97

    UF4G13E0.book  Page 92  Friday, April 27, 2018  3:10 PM

                                                                                 Maintenance

                            EJU33758                              nance not covered by this owner’s/operator’s
                                       Maintenance
                                                                  manual.
                            Periodic  checks and  lubrication will keep  EJU33803
                            your watercraft in the safest and most effi-  Tool kit
                            cient condition  possible. Therefore, make  A tool kit is included with this watercraft. Pla-
                            sure to carry out the periodic maintenance.  ce the tool kit in a waterproof bag and always
                            Safety is an obligation of the watercraft own-  carry it with you whenever you use the water-
                            er. Proper maintenance must be carried out  craft.
                            to keep the exhaust emission and sound lev-
                            els within the regulated limits. The most im-
                            portant points of watercraft inspection  and
                            lubrication are explained on the following pa-
                            ges.
                            See a Yamaha dealer for genuine Yamaha re-
                            placement parts and  optional accessories
                            designed for your watercraft.
                            Remember, failures that are the result of the
                            installation of parts or accessories which are
                                                                   1 Tool bag
                            not qualitatively equivalent  to genuine
                                                                   2 Screwdriver
                            Yamaha parts are not covered by the limited
                                                                   3 Garden hose adapter
                            warranty.
                                                                   4 10/12 mm box wrench
                            Maintenance, replacement, or repair of  5 Pliers
                            the emission control devices and system  6 10/12 mm open-end wrench
                            may be performed by any marine SI engine
                            repair  establishment or individual.  War-
                            ranty repair, however, must be performed
                            at an authorized Yamaha  marine dealer-
                            ship.
                            EWJ00312
                                 WARNING
                            Be sure to turn off the engine when you
                            perform maintenance  unless otherwise
                            specified. If you are not familiar with ma-
                            chine servicing, this work should be done
                            by a Yamaha dealer or other qualified me-
                            chanic.

                            A service  manual is  available for  purchase
                            through a  Yamaha dealer  for owners  who
                            have the mechanical skills, tools, and other
                            equipment necessary to perform  mainte-

                                                                                                   92

| 92 93 94 95 96 97 98 99 100 101 102 |