Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-15
P. 75

    UF4G13E0.book  Page 70  Friday, April 27, 2018  3:10 PM

                                                                    Pre-operation checks

                            EJU32534                              take is clogged, clean it. (See page 100 for in-
                            Fire extinguisher check
                            Check that there is a full fire extinguisher on  formation on the jet intake.)
                                                                  EJU43221
                            board.                                Jet thrust nozzle and reverse gate check
                                                                  (VX / VX Deluxe / VX Cruiser / VX Limited)
                                                                  Check the jet thrust nozzle and reverse gate
                                                                  for damage or other problem.
                                                                  EJU44250
                                                                  Stern drain plug checks
                                                                  Loosen the stern drain plugs and  remove
                                                                  them, and then make sure that the plugs and
                                                                  O-rings on the plugs are not damaged and
                                                                  that there is no foreign material on the
                                                                  threads or O-rings on  the plugs.  NOTICE:
                                                                  Before installing  the stern drain plugs,
                            To check  the  fire extinguisher, see the  in-  clean the  drain plug threads and the  O-
                            structions supplied  by the fire extinguisher  rings on the plugs to remove any foreign
                            manufacturer. Always keep the fire extin-  materials, such as dirt or sand. Otherwise,
                            guisher secured in the holder with its cover in  the stern drain plugs could be damaged,
                            place.                                allowing water to enter the engine com-
                            Always carry a fire extinguisher on board. A  partment. Check the O-rings on the stern
                            fire extinguisher is not standard  equipment  drain plugs and make sure that the plugs
                            with this watercraft. If you do not have one,  are tightened securely before launching
                            contact a Yamaha dealer or a fire extinguish-  the  watercraft. Otherwise, water may
                            er dealer to obtain one meeting the proper  flood the engine compartment and cause
                            specifications.
                                                                  the watercraft to submerge. [ECJ00363]
                              Fire extinguisher:
                                Classification:
                                  B-1
                                Capacity:
                                  2 lb or more

                            EJU40122
                            Safety equipment check
                            Check that safety equipment meeting the ap-
                            plicable regulations is on board.                2
                                                                             1
                            EJU32353
                            Hull and deck check
                                                                   1 Stern drain plug
                            Check the hull and deck for damage or other
                                                                   2 O-ring
                            problem.
                            EJU32657
                            Jet intake checks
                            Make sure that the jet intake is not damaged
                            or clogged with weeds or debris. If the jet in-

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |