Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-15
P. 66

    UF4G13E0.book  Page 61  Friday, April 27, 2018  3:10 PM

                            Operation and handling requirements

                            engine compartment can splash into the  EJU42432 Transporting on a trailer
                            engine, which can result in severe dam-
                                                                  When transporting the watercraft on a trailer,
                            age. [ECJ00554]
                                                                  secure the tie downs to the trailer through the
                                                                  bow eye and stern eyes. NOTICE: Do not at-
                                                                  tach ropes or tie downs to any part of the
                                                                  watercraft  other than  the bow eye  and
                                                                  stern eyes to secure the watercraft to the
                                                                  trailer. Otherwise, the watercraft may be
                                                                  damaged. Wrap the ropes  or  tie  downs
                                                                  with towels or rags where they touch the
                                                                  body of the watercraft to avoid scratches
                                                                  or damage. [ECJ02150]

                            61

| 61 62 63 64 65 66 67 68 69 70 71 |