Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 92 - LIT-18626-12-15
P. 92

    UF4G13E0.book  Page 87  Friday, April 27, 2018  3:10 PM

                            Care and storage

                                ter flows out continually from  the  jet  components to help prevent corrosion.
                                thrust nozzle.                       (See page  90 for  information on rust-
                                                                     proofing the  internal engine  compo-
                                                                     nents.)
                                                                  (3) Rinse  the engine and engine compart-
                                                                     ment with a small amount of  water.
                                                                     NOTICE: Do not use high-pressure
                                                                     water when rinsing the engine or en-
                                                                     gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (4) Drain  the water  from the engine com-
                                                                     partment. (See page 60 for information
                            (7) Run the engine at idling speed for about  on draining the bilge water.)
                                3 minutes watching the engine condition.  (5) Wipe  the engine  and engine compart-
                                If the  engine stops  while flushing,  turn  ment with a dry cloth.
                                the water supply off immediately  and  (6) Wash down the hull, deck, and jet pump
                                perform the procedure again from step 6.  with fresh water.
                                NOTICE: Do not supply water to the  (7) Wipe the hull, deck, and jet pump with a
                                cooling water passages when the en-  dry cloth.
                                gine is not running. The water could  (8) Wipe  all vinyl and rubber components,
                                flow back through the muffler into the  such as the seats and engine compart-
                                engine, causing severe engine  dam-  ment seals, with a vinyl protectant such
                                                                     as Yamaclean Vinyl Dressing™.
                                age. [ECJ00123]
                            (8) Turn the water supply off.        (9) To minimize corrosion, spray metallic
                            (9) Discharge the remaining water out of the  parts of the hull, deck, and engine with a
                                cooling  water passages by  alternately  rust inhibitor such as Yamalube Silicone
                                squeezing and releasing the throttle lever  Protectant & Lubricant.
                                quickly for 10 to 15 seconds.     (10) Allow the engine compartment to air dry
                            (10) Stop the engine.                    completely before installing the seats.
                            (11) Remove the garden hose adapter, and  (11) Securely install the seats in their original
                                then securely install the flushing hose  positions.
                                connector cap  by tightening  it until it  EJU41632
                                                                  Battery care
                                stops.
                                                                  If the watercraft will not be used for more than
                            (12) Securely install the removable watertight
                                                                  a month, remove the battery from the water-
                                storage compartment and seats in their
                                                                  craft, check it, and then store it in a cool, dry
                                original positions.
                                                                  place.
                            EJU43931
                            Cleaning the watercraft               EWJ00792
                            (1) Remove the seats. (See page 49 for seat  WARNING
                                removal and installation procedures.)  Battery electrolyte is poisonous and dan-
                            (2) If the watercraft will be stored for a week  gerous, causing severe burns, etc. Elec-
                                or more,  rustproof  the internal engine

                            87

| 87 88 89 90 91 92 93 94 95 96 97 |