Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 22 - LIT-18626-12-15
P. 22

    UF4G13E0.book  Page 17  Friday, April 27, 2018  3:10 PM

                                Safety information

                              help keep the watercraft from moving in ei-  contact with the rotating parts of the jet
                              ther  direction, although some  movement  pump.
                              may occur.

                                                                                                 2

                                                                                         1

                                             1                     1 Intake grate
                              1 “N” (Neutral position)             2 Jet thrust nozzle
                             VX / VX Deluxe / VX Cruiser / VX Limited:    Stop the engine and remove the clip from
                              To avoid rear-end collisions while operat-  the engine shut-off switch before removing
                              ing the watercraft, check behind you be-  any debris or weeds, which may have col-
                              fore using the RiDE lever to slow down or  lected around the jet intake.
                              stop the watercraft. Make sure that there                  2
                              are no obstacles or people behind you be-
                              fore shifting into reverse.
                             Keep away from the intake grate while the
                              engine is on. Items such as long hair, loose
                              clothing, or PFD straps can become entan-                       1
                              gled in moving parts, resulting in severe in-
                              jury or drowning.
                             Never insert any object into the jet thrust
                              nozzle while the engine is running. Severe
                              injury or death could result from coming in  1 Clip
                                                                   2 Engine shut-off switch

                            17

| 17 18 19 20 21 22 23 24 25 26 27 |