Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 106 - LIT-18626-12-15
P. 106

    UF4G13E0.book  Page 101  Friday, April 27, 2018  3:10 PM

                            Trouble recovery

                                ler, jet pump housing, and jet thrust noz-  (4) Raise the reverse gate to the forward po-
                                zle.                                 sition.
                                If debris is difficult to remove, consult a
                                Yamaha dealer.
                            EJU43472
                            Raising the reverse gate (VX /
                            VX Deluxe / VX Cruiser / VX Limited)
                            If the RiDE system malfunctions and the re-       1
                                                                                               2
                            verse gate remains in the lowered position,
                            the watercraft will not be able to move for-
                            ward.
                            After raising the reverse gate so that the wa-
                            tercraft can move  forward, immediately  re-  1 Reverse gate
                            turn to shore and have a  Yamaha dealer  2 Forward position
                            service the watercraft.
                                                                  TIP:
                            To raise the reverse gate:
                            (1) Stop the engine and remove the clip from   While the shift rod is disconnected, the re-
                                the engine shut-off switch.        verse gate will not move to the neutral po-
                            (2) Enter the water and move to the rear of  sition or reverse position even if the RiDE
                                the watercraft.                    lever is squeezed.
                            (3) Slide the shift rod joint toward the bow,   If the RiDE lever is squeezed while the shift
                                and then disconnect the shift rod joint  rod is disconnected, the watercraft will
                                from the ball joint.               move forward.
                                                                  EJU34642
                                                                  Jumping the battery
                                                                  If the watercraft battery has run down, the en-
                                                                  gine can be started using a 12-volt booster
                                                                  battery and jumper cables.
                                                                  EJU34664
                                                  1        2      Connecting the jumper cables
                                                                  EWJ01251
                                                                      WARNING
                                                                  To avoid battery explosion  and serious
                                                                  damage to the electrical system:
                              1 Shift rod joint                    Do not reverse the polarity of the jumper
                              2 Ball joint                         cables when connecting to the batter-
                                                                   ies.
                                                                   Do not connect the negative (–) jumper
                                                                   cable to the negative (–) terminal of the
                                                                   watercraft battery.
                                                                   Do not touch the positive (+) jumper ca-
                                                                   ble to the negative (–) jumper cable.

                            101

| 101 102 103 104 105 106 107 108 109 110 111 |