Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-15
P. 69

    UF4G13E0.book  Page 64  Friday, April 27, 2018  3:10 PM

                                                                    Pre-operation checks

                                      ITEM                         ROUTINE                   PAGE
                             Jet thrust nozzle and re-
                             verse gate  (VX / VX   Check the jet thrust nozzle and reverse gate for   70
                             Deluxe / VX Cruiser / VX   damage.
                             Limited)
                                                    Check the stern drain plugs for damage and foreign
                             Stern drain plugs                                                70
                                                    material and check that they are securely installed.
                             Hood                   Check that the hood is securely closed.   71
                             Front and rear seats   Check that the seats are securely installed.  49
                             POST-LAUNCH CHECKS
                                                    Check that water is discharged from the cooling
                             Cooling water pilot outlet                                       71
                                                    water pilot outlet while the engine is running.
                             Multifunction information   Check the multifunction information center for prop-  71
                             center                 er operation.
                             Shift system (VX /
                             VX Deluxe / VX Cruiser / VX  Check the shift system for proper operation.  71
                             Limited)
                             Engine idling speed    Check the engine idling speed.            72
                            TIP:
                            To ensure safety and reliability, pre-operation checks should be made each time the water-
                            craft is used.

                                                                                                   64

| 64 65 66 67 68 69 70 71 72 73 74 |