Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-15
P. 64

    UF4G13E0.book  Page 59  Friday, April 27, 2018  3:10 PM

                            Operation and handling requirements

                             When checking the engine oil level on wa-  engine oil level is between the minimum
                              ter, moor the watercraft so that it will not  and maximum level marks.
                              drift away.
                            To check the engine oil level:
                            (1) With the engine stopped, place the wa-
                                tercraft in  a precisely level position on
                                land or launch the watercraft.
                            (2) Look in all directions, and then start the
                                engine. (See page 74 for information on
                                starting the engine.)                     1    2      3
                            (3) Run the engine at idling speed for 6 mi-
                                nutes or more. Run the engine an addi-
                                tional 5  minutes if the ambient   1 Dipstick
                                                                   2 Maximum level mark
                                temperature is 20 °C (68 °F) or less.
                                                                   3 Minimum level mark
                            (4) Stop the engine.
                            (5) Remove the seats. (See page 49 for seat  (8) If the engine oil  level  is  significantly
                                removal and installation procedures.)  above the maximum level mark, consult
                            (6) Loosen the oil tank filler cap and remove  a Yamaha dealer. If the engine oil level is
                                it, and then wipe  the attached dipstick  below the minimum  level mark,  slowly
                                clean.                               add engine oil.
                                                                  (9) Repeat steps 6–8 until the engine oil is at
                                                                     the proper level.
                                                                  (10) Securely install the oil tank filler cap and
                                                                     turn it until it stops.
                                                                  (11) Securely install the seats in their original
                                                        1
                                                                     positions.

                              1 Oil tank filler cap/Dipstick
                            (7) Screw the oil tank filler cap into the filler
                                hole until it stops. Remove the oil tank
                                filler cap again and make sure that the

                            59

| 59 60 61 62 63 64 65 66 67 68 69 |