Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-12-15
P. 37

    UF4G13E0.book  Page 32  Friday, April 27, 2018  3:10 PM

                                                             Control function operation

                            two conditions: (1) this device may not cause
                                                                                               “UN-
                            harmful interference, and (2) this device must  Number of   Yamaha Security  LOCK” in-
                            accept  any interference received, including  beeps  System mode  dicator
                                                                                               light
                            interference that may cause undesired oper-
                            ation.                                                 Lock       Goes off
                            ECJ00031                                              Unlock      Comes
                             NOTICE                                           (normal operation   on
                                                                                  mode)
                            Changes or modifications not  expressly
                                                                                  Unlock      Comes
                            approved by the party responsible for             (Low RPM Mode)    on
                            compliance could void the user’s authority
                            to operate the remote control transmitter.  TIP:
                                                                   The beeper sounds two times for the nor-
                            EJU31385
                            Yamaha Security System (VX Deluxe /    mal operation mode or three times for the
                            VX Cruiser / VX Limited)               Low RPM Mode. (See  page 39  for Low
                            The  Yamaha  Security System functions to  RPM Mode activation procedures.)
                            help prevent unauthorized use or theft of the   If the remote control transmitter is operated
                            watercraft. The lock and unlock modes of the  while the multifunction information center
                            security system can be selected by operating  is in the standby state, the center will per-
                            the remote control transmitter that is included  form the initial operation, and then the set-
                            with  this watercraft. The engine  cannot  be  ting is selected.
                            started if the lock mode of the security sys-  To select the lock mode:
                            tem is selected. The engine can only be start-  Push the lock button on the remote control
                            ed if the unlock mode is selected. (See page  transmitter briefly. The beeper sounds once
                            31 for information on the remote control  and the “UNLOCK” indicator light  blinks
                            transmitter.)                         once, then goes off. This indicates the lock
                                                                  mode is selected.
                            TIP:
                            The  Yamaha  Security System settings can                            2
                                                                        1
                            only be selected while the engine is stopped.
                            EJU36776
                            Yamaha Security System settings
                            The Yamaha Security System settings will be
                            confirmed by the number of beeps when the
                            remote control transmitter is operated, and
                            by the “UNLOCK” indicator light of the multi-
                            function information center. (See page 44 for
                            information on the multifunction information
                            center.)                               1 Lock button
                                                                   2 “UNLOCK” indicator light
                                                                  To select the unlock mode:
                                                                  Push the “L-Mode” (unlock) button on the re-
                                                                  mote control transmitter briefly. The beeper
                                                                  sounds two  or  three times  and the “UN-

                                                                                                   32

| 32 33 34 35 36 37 38 39 40 41 42 |