Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - LIT-18626-12-15
P. 76

    UF4G13E0.book  Page 71  Friday, April 27, 2018  3:10 PM

                            Pre-operation checks

                            Securely install the stern drain plugs by tight-  running. (See page 35 for information on the
                            ening them until they stop.           cooling water pilot outlet.)

                                           1

                              1 Stern drain plug
                                                                  EJU32715
                                                                  Multifunction information center check
                            EJU43810
                            Hood check                            Make sure that the multifunction information
                            Push down the hood latch and make sure  center operates properly. (See page 44 for in-
                            that it is securely closed.           formation on proper operation of the multi-
                                                                  function information center.)

                            EJU40146
                            Post-launch checks
                                                                  EJU43392
                            Perform the post-launch checks in the pre-  Shift system check (VX / VX Deluxe /
                            operation checklist while the watercraft is in  VX Cruiser / VX Limited)
                            the water and the engine is running.  Operate the throttle lever and RiDE lever, and
                            To perform the post-launch checks:    check that the watercraft moves or does not
                            (1) Launch the watercraft. (See page 74 for  move according to the displayed shift indica-
                                information on launching the watercraft.)  tor. (See page 37 for shift system operation
                            (2) Perform the checks and make sure that  procedures.)  WARNING! To avoid colli-
                                there are no malfunctioning items or oth-  sions, operate at safe speeds and keep a
                                er problems.
                            EJU40553
                            Cooling water pilot outlet check
                            Make sure that water is discharged from the
                            cooling water pilot outlet while the engine is

                            71

| 71 72 73 74 75 76 77 78 79 80 81 |