Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-12-15
P. 81

    UF4G13E0.book  Page 76  Friday, April 27, 2018  3:10 PM

                                                                                      Operation

                            dental starting or unauthorized operation by  (idle) position. (See page 37 for shift system
                            children or others.                   operation procedures.)

                                                                                   1
                                                                   1 “F” (Forward position)
                            EJU44990
                            Operating the watercraft
                            VX-C:
                            When the engine  is  running, the watercraft
                            will move forward at trolling speed even if the
                            throttle lever is in the fully closed (idle) posi-
                            tion.

                                                                  EJU43422
                                                                  Turning the watercraft
                                                                  EWJ01782
                                                                      WARNING
                                                                   Do not release the throttle lever when
                                                                   trying to steer away from objects—you
                            VX / VX Deluxe / VX Cruiser / VX Limited:   need throttle to steer. A collision could
                            When the throttle lever is squeezed, the “F”  result in severe injury or death.
                            (forward) shift indicator will be displayed and   When operating at higher speeds, make
                            the watercraft will move forward. While the  gradual turns or slow down before turn-
                            “F” (forward) shift indicator is displayed, the  ing. Sharp high-speed turns may cause
                            watercraft will move forward at trolling speed  the watercraft to slide sideways or spin,
                            even if the throttle lever is in the fully closed  throwing the operator and passenger(s)
                                                                   overboard, which could cause an injury.
                                                                   VX / VX Deluxe / VX Cruiser / VX Limited:
                                                                   Take early action to avoid collisions. The
                                                                   RiDE system is not a braking device for
                                                                   avoiding dangerous situations.

                                                                                                   76

| 76 77 78 79 80 81 82 83 84 85 86 |