Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-15
P. 39

    UF4G13E0.book  Page 34  Friday, April 27, 2018  3:10 PM

                                                             Control function operation

                            in 5 seconds, release the start switch, wait 15  EJU31212
                                                                  Throttle lever
                            seconds, and then try again. NOTICE: Never
                                                                  The throttle lever increases the engine speed
                            push the start switch while the engine is
                                                                  when the lever is squeezed.
                            running. Do not operate the start switch
                            for  more than 5 seconds, otherwise the
                            battery will be discharged and the engine     1
                            will not start. Also, the starter motor could
                            be damaged. [ECJ01041]

                                                     1

                                                                   1 Throttle lever
                                                                  The throttle lever returns automatically to its
                                                                  fully closed (idle) position when released.
                                                                  EJU43342
                                                                  RiDE lever (VX / VX Deluxe /
                              1 Start switch
                                                                  VX Cruiser / VX Limited)
                            The engine will not start under any of the fol-  When the RiDE lever is squeezed, the reverse
                            lowing conditions:                    gate lowers and the watercraft starts moving
                             Clip is removed  from  the engine  shut-off  in reverse. If the watercraft is moving forward,
                              switch.                             the watercraft gradually slows down until it
                             Throttle lever is squeezed.         stops, and then the watercraft starts moving
                             Throttle lever is malfunctioning.   in reverse.
                             VX / VX Deluxe / VX Cruiser / VX Limited:
                              RiDE lever is squeezed.                                 1
                             VX / VX Deluxe / VX Cruiser / VX Limited:
                              RiDE lever is malfunctioning.
                             VX Deluxe / VX Cruiser / VX Limited: Lock
                              mode of the Yamaha Security System has
                              been selected. (See page 32 for Yamaha
                              Security System setting procedures.)

                                                                   1 RiDE lever
                                                                  When the RiDE lever is released, it automati-
                                                                  cally returns to its fully closed (idle) position
                                                                  and the reverse gate moves to the neutral po-
                                                                  sition.

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |