Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-12-16
P. 45

    UF3Y12E0.book  Page 40  Friday, April 27, 2018  1:38 PM

                                                                     Instrument operation

                            To switch the speedometer display units:  EJU44650
                                                                  Tachometer
                            Start the engine, stop the engine, and then
                                                                  The tachometer shows the engine speed.
                            push the engine stop switch 3 times, pushing
                            the switch for 0.4 seconds or more each time,                1
                            before the  multifunction information center
                            turns  off. The speedometer display  units
                            change.
                            To  switch the speedometer display units
                            again, repeat this procedure.

                                                                   1 Tachometer
                                                                  TIP:
                                                                  While the engine is stopped, the battery volt-
                                                                  age and the total engine hours are displayed
                                                 1                alternately.
                                                                  EJU43891
                                                                  Shift indicator (EX Deluxe)
                              1 Engine stop switch
                                                                  This indicator shows the  reverse  gate shift
                                                                  positions: “F” (forward), “N” (neutral), and “R”
                                                                  (reverse).  (See page 35 for shifting proce-
                                                                  dures.)
                                                                               1
                                                                                                  2
                                                                                                  3

                                                                                                  4
                                                1
                              1 Speedometer

                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU44700
                                                                  Hour meter and voltmeter
                                                                  The hour meter and voltmeter are displayed
                                                                  in the tachometer portion of the information
                                                                  display while the engine is stopped.

                                                                                                   40

| 40 41 42 43 44 45 46 47 48 49 50 |