Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - LIT-18626-12-16
P. 41

    UF3Y12E0.book  Page 36  Friday, April 27, 2018  1:38 PM

                                                                      Watercraft operation

                             Do not touch the reverse gate while the  reverse, and the “R” (reverse) shift indi-
                              RiDE lever is being operated, otherwise  cator will be displayed.
                              you could be pinched.
                             If the RiDE  lever and throttle lever are               1
                              being operated at the same time, do not
                              release only the RiDE lever. Otherwise,
                              the watercraft  could accelerate more
                              quickly than expected, which may lead
                              to an accident.

                            The RiDE lever and throttle lever can be oper-
                            ated to change the forward or rearward
                            movement of the watercraft only when the  1 RiDE lever
                            engine is running.  When the  RiDE  lever is
                            squeezed, the reverse gate lowers and de-
                            flects the water jet being discharged from the               1
                            jet thrust nozzle so that the watercraft moves
                            in reverse or is in neutral. When the throttle le-
                            ver is squeezed, the reverse gate rises and
                            the watercraft moves forward.
                            TIP:
                             This  model is equipped with a function                           2
                              which limits the engine speed in reverse.
                             When the  engine is started,  the reverse  1 Reverse gate
                              gate automatically moves to the neutral po-  2 Reverse position
                              sition.
                            To shift into reverse:                             1
                            (1) Release the throttle lever.
                            (2) Squeeze the  RiDE lever. The reverse
                                gate will lower, the engine speed will in-
                                crease, the watercraft will start moving in

                                                                   1 “R” (Reverse position)
                                                                  To shift into neutral from reverse:
                                                                  Release the RiDE lever. The reverse gate will
                                                                  automatically return to the  neutral position

                                                                                                   36

| 36 37 38 39 40 41 42 43 44 45 46 |