Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-12-16
P. 83

    UF3Y12E0.book  Page 78  Friday, April 27, 2018  1:38 PM

                                                                                      Operation

                            EX Deluxe:                             Do not put your hands in the intake
                            (1) Launch the watercraft.             grate.
                            (2) Attach the engine shut-off cord (lanyard)
                                                                  If the watercraft capsizes, turn it over imme-
                                to your left wrist, and then attach the clip
                                                                  diately.
                                to the engine shut-off switch.
                                                                  To upright the watercraft:
                            (3) Look in all directions, and then start the
                                                                  (1) Remove the clip from the engine shut-off
                                engine.
                                                                     switch.
                            (4) Squeeze the RiDE lever and  move the
                                                                  (2) Swim to the rear of the watercraft. Turn
                                watercraft back slowly. (See page 35 for
                                                                     the watercraft over by pulling on the ride
                                RiDE lever operation procedures.)
                                                                     plate with one hand while pushing down
                            EJU33114
                            Boarding and starting off from a dock    on the gunwale with your other hand or
                            (1) Board the watercraft from the side.  your foot.
                            (2) Attach the engine shut-off cord (lanyard)
                                to your left wrist, and then attach the clip
                                to the engine shut-off switch.
                            (3) Push the watercraft away from the dock,
                                grip the handlebars with both hands, and
                                place both feet on the floor of the foot-
                                well.

                            (4) Look in  all  directions, start the engine,
                                and then start off slowly.
                            EJU44210
                            Capsized watercraft
                            EWJ00672                              (3) Start the engine and operate the water-
                                 WARNING                             craft at planing speed to drain the bilge
                            Improper uprighting can cause injury.    water  from the engine  compartment.
                             Be sure to shut the engine off by pulling  (See page 53 for information on draining
                              on the engine shut-off cord (lanyard) to  the bilge water. If the engine does not
                              remove the clip from the engine shut-off  start, see “Towing  the  watercraft” on
                              switch.                                page 98 or “Submerged watercraft” on
                                                                     page 98.) NOTICE: Do not run the en-
                                                                     gine at full throttle for at least 1 minute

                                                                                                   78

| 78 79 80 81 82 83 84 85 86 87 88 |