Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 71 - LIT-18626-12-16
P. 71

    UF3Y12E0.book  Page 66  Friday, April 27, 2018  1:38 PM

                                                                    Pre-operation checks

                            EJU43392
                            Shift system check (EX Deluxe)
                            Operate the throttle lever and RiDE lever, and
                            check that the watercraft moves or does not
                            move according to the displayed shift indica-
                            tor. (See page 35 for shift system operation
                            procedures.)  WARNING! To avoid colli-
                            sions, operate at safe speeds and keep a
                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]
                                         1
                                                             2

                                                             3

                                                             4

                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.

                              Engine idling speed:
                                1500 ±100 r/min

                                                                                                   66

| 66 67 68 69 70 71 72 73 74 75 76 |