Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - LIT-18626-12-17
P. 68

    UF4L10E0.book  Page 63  Tuesday, July 10, 2018  1:34 PM

                            Pre-operation checks

                            er dealer to obtain one meeting the proper  flood the engine compartment and cause
                            specifications.                       the watercraft to submerge. [ECJ00363]
                              Fire extinguisher:
                                Classification:
                                  B-1
                                Capacity:
                                  2 lb or more

                            EJU40122
                            Safety equipment check
                            Check that safety equipment meeting the ap-
                            plicable regulations is on board.                2
                            EJU32353                                         1
                            Hull and deck check                    1 Stern drain plug
                            Check the hull and deck for damage or other  2 O-ring
                            problem.
                                                                  Securely install the stern drain plugs by tight-
                            EJU32657
                            Jet intake checks                     ening them until they stop.
                            Make sure that the jet intake is not damaged
                            or clogged with weeds or debris. If the jet in-
                            take is clogged, clean it. (See page 91 for in-
                            formation on the jet intake.)
                            EJU43221
                            Jet thrust nozzle and reverse gate check
                            Check the jet thrust nozzle and reverse gate         1
                            for damage or other problem.
                            EJU44250
                            Stern drain plug checks
                            Loosen  the stern  drain plugs and remove
                            them, and then make sure that the plugs and  1 Stern drain plug
                            O-rings on the plugs are not damaged and  EJU44640
                                                                  Hood check
                            that there is no foreign material  on  the
                            threads or O-rings  on  the plugs.  NOTICE:  Close the hood, hook the hood latches, and
                                                                  check that the hood is securely closed.
                            Before installing the stern drain plugs,
                            clean the drain plug threads and the O-
                            rings on the plugs to remove any foreign
                            materials, such as dirt or sand. Otherwise,
                            the stern drain plugs could be damaged,
                            allowing water to enter the engine com-
                            partment. Check the O-rings on the stern                           1
                            drain plugs and make sure that the plugs
                            are tightened securely before launching
                            the  watercraft. Otherwise, water may
                                                                   1 Hood latch

                            63

| 63 64 65 66 67 68 69 70 71 72 73 |