Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 87 - LIT-18626-12-17
P. 87

    UF4L10E0.book  Page 82  Tuesday, July 10, 2018  1:34 PM

                                                                           Care and storage

                            To rustproof the internal engine components:  engine is hot. The sprayed substance
                            (1) Remove  the seat and  fire extinguisher  or propellants could catch fire. [EWJ00262]
                                holder. (See page 43 for seat  removal
                                and installation procedures and page 48
                                for information on  the fire extinguisher
                                holder.)
                            (2) Remove the plastic tie that is fastening
                                the fuel hose to the holder on the star-      1
                                board side of the air filter case.
                            (3) Release the hooks on the port side of the
                                air filter case, and  remove the air filter
                                case cover.
                                                                   1 Intake opening
                                         2                        (5) Place the air filter case cover in its origi-
                                                             3
                              1                                      nal position, and then fit the hooks onto
                                                             4       the cover.
                                                             5    TIP:
                                                                  Make sure that the air filter case cover is se-
                                                                  curely installed.
                                                                  (6) Fasten the fuel hose to the holder using
                                                                     the plastic tie.
                                                                  (7) Make sure that the area around the wa-
                                                                     tercraft is clear, and then start the engine
                                                                     in a well-ventilated area and let it run at
                                                                     idle for 15 seconds. (See page 31 for in-
                                                                     formation on starting the engine.)
                                                                  (8) Stop the engine.
                                                                  (9) Securely install the fire extinguisher hold-
                                                                     er and seat in their original positions.

                              1 Hook
                              2 Air filter case cover
                              3 Fuel hose
                              4 Holder
                              5 Plastic tie
                            (4) Spray a rust inhibitor such as Yamalube
                                Stor-Rite Engine Fogging Oil into the in-
                                take opening for 3 seconds. WARNING!
                                Do not spray flammable rust inhibitor
                                products on engine surfaces while the

                                                                                                   82

| 82 83 84 85 86 87 88 89 90 91 92 |