Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-17
P. 63

    UF4L10E0.book  Page 58  Tuesday, July 10, 2018  1:34 PM

                                                                    Pre-operation checks

                            EJU32282                              Make sure that there is no damage inside the
                               Pre-operation check points
                                                                  engine compartment.
                            EJU44550
                            Pre-launch checks
                            Perform the pre-launch checks in the pre-op-
                            eration checklist while the watercraft is  on
                            land.
                            To perform the pre-launch checks:
                            (1) Remove the seat, seat storage compart-
                                ment, and fire extinguisher holder. (See
                                page 43 for seat removal and installation
                                procedures, page 47 for information on
                                the seat storage compartment, and page
                                48 for information on the fire extinguisher  EJU34215
                                                                  Fuel system checks
                                holder.)                          EWJ00382
                            (2) Perform the checks and make sure that  WARNING
                                there are no malfunctioning items or oth-  Leaking fuel can result in fire or explosion.
                                er problems.                       Check for fuel leakage regularly.
                            (3) After completing these checks, securely   If any fuel leakage is found, the fuel sys-
                                install the seat storage compartment, fire  tem must be repaired by a qualified me-
                                extinguisher holder, and seat in their  chanic. Improper repairs can make the
                                original positions.                watercraft unsafe to operate.
                            EJU32334
                            Engine compartment check              Make sure that there is no damage, leakage,
                            EWJ00462
                                 WARNING                          or other problem in the fuel system.
                                                                  Check:
                            Failure  to  ventilate the engine compart-
                                                                   Fuel filler cap and seal for damage
                            ment could result in a fire or explosion. Do
                                                                   Fuel tank for damage and leakage
                            not start the engine if there is a fuel leak.
                                                                   Fuel hoses and joints for damage and leak-
                            Ventilate the engine compartment. Leave the  age
                            engine compartment open for a few minutes   Fuel tank breather hose  for damage and
                            to allow any fuel vapors to escape.    leakage
                                                                  EJU36875
                                                                  Fuel level check
                                                                  Check the fuel level in the fuel tank.
                                                                  Add fuel if necessary. (See page 49 for infor-
                                                                  mation on filling the fuel tank.)
                                                                  EJU32424
                                                                  Water separator check
                                                                  Make sure that no water has collected in the
                                                                  water separator. If water has collected in the

                                                                                                   58

| 58 59 60 61 62 63 64 65 66 67 68 |