Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-12-17
P. 58

    UF4L10E0.book  Page 53  Tuesday, July 10, 2018  1:34 PM

                            Operation and handling requirements

                                drain plugs could be damaged, allow-  engine compartment can splash into the
                                ing water to enter the engine compart-  engine, which can  result in severe  dam-
                                ment. Check the O-rings on the stern  age. [ECJ00554]
                                drain plugs  and make  sure that  the
                                plugs are tightened  securely before
                                launching the watercraft. Otherwise,
                                water may flood the engine compart-
                                ment and cause the watercraft to sub-
                                merge. [ECJ00363]

                                                  1

                              1 O-ring
                            (5) Securely install the stern drain plugs by
                                tightening them until they stop.
                            EJU40535
                            Draining the bilge water on water
                            A small quantity of bilge water will remain in
                            the engine compartment even after the bilge
                            water is drained on  water. To  completely
                            drain the bilge water, remove the watercraft
                            from the water and drain the bilge water on
                            land.
                            Jet vacuum bilge draining system
                            While the watercraft is operating, bilge water
                            in the engine compartment is drawn in by the
                            vacuum that is generated in the jet pump and
                            discharged from the watercraft through the
                            jet thrust nozzle.
                            To drain the bilge water on water:
                            Operate the watercraft as straight as possible
                            and above planing speed for at least 2 minu-
                            tes. NOTICE: Do not run the engine at full
                            throttle for at least 1 minute after the en-
                            gine has been restarted. Bilge water in the

                            53

| 53 54 55 56 57 58 59 60 61 62 63 |