Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - LIT-18626-12-17
P. 41

    UF4L10E0.book  Page 36  Tuesday, July 10, 2018  1:34 PM

                                                                      Watercraft operation

                            and the “N” (neutral) shift indicator will be dis-  To shift into forward:
                            played.                               (1) Release the RiDE lever.
                                                                  (2) Squeeze the throttle lever. The reverse
                                                                     gate  will rise completely, the engine
                                               1
                                                                     speed will increase, the watercraft will
                                                                     start moving forward, and the “F” (for-
                                                                     ward) shift indicator will be displayed.

                                                                          1

                              1 RiDE lever

                                                    1

                                                                   1 Throttle lever

                                                                                         1
                                                          2

                              1 Reverse gate                                                   2
                              2 Neutral position

                                         1

                                                                   1 Reverse gate
                                                                   2 Forward position

                                                                               1

                              1 “N” (Neutral position)
                            TIP:
                            Although the neutral position helps keep the
                            watercraft from moving even when the en-
                            gine is running, some movement may occur.
                                                                   1 “F” (Forward position)

                                                                                                   36

| 36 37 38 39 40 41 42 43 44 45 46 |