Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 29 - LIT-18626-12-56
P. 29

    Control function operation

           EJU31026                             vent accidental starting or unauthorized op-
            Watercraft control functions
                                                eration by children or others.
           EJU31153
           Engine stop switch “ ”
           The engine stop switch (red button) stops the
           engine when the switch is pushed.

                                                EJU41051
                                                Start switch “  ”
                                     1          ECJ01361
                                                 NOTICE
            1 Engine stop switch
                                                Do not run  the engine for  more than 15
           EJU31164
           Engine shut-off switch “  ”          seconds on land without supplying water,
           The  engine shut-off switch  automatically  otherwise the engine could overheat.
           stops the engine when the clip, on the end of
                                                The start switch (green button) starts the en-
           the engine shut-off cord (lanyard), is removed
                                                gine when the switch is pushed.
           from the switch, such as if the operator falls
                                                Release the start switch as soon as the en-
           off the watercraft.
                                                gine starts to run. If the engine does not start
           Insert the clip  under the engine  shut-off
                                                in 5 seconds, release the start switch, wait 15
           switch before starting the engine.
                                                seconds, and then try again. NOTICE: Never
                                                push the start switch while the engine is
                        1          2
                                                running. Do not operate the start switch
                                                for  more than 5  seconds, otherwise  the
                                                battery will be discharged and the engine
                           STOP
                     3

            1 Engine shut-off switch
            2 Clip
            3 Engine shut-off cord (lanyard)
           When the engine is not running, remove the
           clip from the engine shut-off switch to pre-

                                                                                 22

| 24 25 26 27 28 29 30 31 32 33 34 |