Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 35 - LIT-18626-12-56
P. 35

    Equipment operation

           To remove the storage pouch:         To open the fire extinguisher container:
           (1) Remove the hood. (See page 26 for hood  (1) Lift the steering pole and support it with
              removal and installation procedures.)  the lock pin.
           (2) Unfasten the  bands,  and then remove
              the storage pouch.

                                                  1 Steering pole
                                                  2 Lock pin
            1 Storage pouch                     (2) Grasp the tab, pull the band to the rear,
            2 Band
                                                   and then pull it up.
           To install the storage pouch:
           (1) Bend the owner’s/operator’s manual
              slightly to insert it into the storage pouch,
              and then add the tool kit and any other
              small items. Fold the pouch, and  then
              wrap the strap around it.

                                                  1 Fire extinguisher container
                                                  2 Tab
                                                (3) Lift the fire extinguisher container about
                                                   30  degrees  from the storage position.
                                                   NOTICE: Do not force  the  fire extin-
                                                   guisher container up more than 30 de-
            1 Strap                                grees from the storage position,
           (2) Install the  storage  pouch on the hood  otherwise the container and hood
              and secure it with the bands.        could be damaged. [ECJ00402]
           (3) Securely install the  hood in its original
              position.
           EJU41004
           Fire extinguisher container
           The fire extinguisher container is located on
           the hood.

                                                                                 28

| 30 31 32 33 34 35 36 37 38 39 40 |