Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-56
P. 46

    Pre-operation checks

           Add fuel if necessary. (See page 31 for infor-  aged, obstructed, or not connected prop-
           mation on filling the fuel tank.)    erly. [EWJ00452]
           EJU32424
           Water separator check
           Make sure that no water has collected in the
           water separator. If water has collected in the
           water separator, drain it. (See page 25 for in-
           formation on draining the water separator.)

                     1
                     2
                                                  1 Positive (+) battery terminal: Red lead
                                                  2 Negative (–) battery terminal: Black lead
                                                  3 Breather hose
                                                Make sure  that the electrolyte level is be-
                                                tween the minimum and maximum level
                                                marks. WARNING! Never operate the wa-
            1 Water separator
            2 Drain screw                       tercraft if the battery does not have suffi-
                                                cient  power to  start the engine or if  it
           EJU40182
           Engine unit check                    shows any other signs of decreased pow-
           Check the exterior of the engine unit for dam-  er. Loss of battery power may leave you
           age or other problem.                stranded. [EWJ01241]
           EJU41012
           Bilge water check
           Make sure that no bilge water has collected in
           the engine compartment. If bilge water has
           collected in the engine compartment, wipe it
           up with a dry cloth. NOTICE: Excessive wa-
           ter in the engine compartment can splash
           into the engine, which can result in severe
           damage. [ECJ00342]
           EJU32485
           Battery checks
           Make  sure that  the battery terminals and  1 Maximum level mark
           breather hose are not damaged and that the  2 Minimum level mark
           battery leads and breather hose are connect-  Make sure that the battery is securely held in
           ed properly.  WARNING! Fire or explosion  place.
           could result if the breather hose is dam-  EJU32614
                                                Steering system checks
                                                Turn the handlebars to the right and left sev-
                                                eral times  to  make sure that operation is
                                                smooth and unrestricted throughout the

           39

| 41 42 43 44 45 46 47 48 49 50 51 |