Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-12-56
P. 54

    Operation

              lision or  cause the operator to be  dental starting or unauthorized operation by
              thrown overboard. [EWJ00592]      children or others.

                              START                               STOP

           (6) After the engine has warmed up, push  EJU41172
                                                Operating the watercraft
              the choke knob in to its original position.
                                                When the  engine is running, the  watercraft
           TIP:                                 will move forward at trolling speed even if the
           If the choke knob is left pulled out, the engine  throttle lever is in the fully closed (idle) posi-
           will stall.                          tion.
           EJU32863
           Stopping the engine
           Release the throttle lever, and then push the
           engine stop switch (red button) to stop the
           engine.  WARNING!  You need throttle  to
           steer. Shutting  the engine off can  cause
           you to hit an obstacle you are attempting
           to avoid. A collision could result in severe
           injury or death. [EWJ00602]

                                                EJU33245
                                                Turning the watercraft
                                                EWJ00763
                                                    WARNING
                                                z Do not release the throttle lever when
                                                  trying to  steer away from  objects—as
                                                  with other powerboats, you need throt-
                                                  tle to steer. A collision could result in se-
                                                  vere injury or death.
           EJU32873                             z When operating at higher speeds, make
           Leaving the watercraft
                                                  gradual turns or slow down before turn-
           If leaving the watercraft, remove the clip from
                                                  ing. Sharp high-speed turns may cause
           the  engine shut-off switch  to prevent  acci-
                                                  the watercraft to slide sideways or spin,

           47

| 49 50 51 52 53 54 55 56 57 58 59 |