Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 31 - LIT-18626-12-56
P. 31

    Control function operation

           EJU31124                             fuel while operating the watercraft. When this
           Fuel cock knob
                                                occurs, refuel as soon as possible and be
           The fuel supply method can be switched by
                                                sure to turn the fuel cock knob back to “ON”.
           operating the fuel cock knob.
                                                EJU31203
           Select the fuel cock knob position from the  Choke knob “  ”
           following three positions according to the cir-  The choke knob can be operated to supply a
           cumstances of use.                   richer air-fuel mixture that is required to start
                                                a cold engine.
                                                To use the choke:
                                                Pull the choke knob out.
                                                Push the  choke knob  in  to stop using the
                                                choke after the engine starts.

            1 Fuel cock knob

                                                  1 Choke knob
                                                EJU31224
                                                Cooling water pilot outlet
                                                When the engine  is running, some of the
                                                cooling water that is circulated in the engine
                                                is discharged from  the cooling  water pilot
                                                outlet.
           OFF:
           With the fuel cock knob in this position, fuel
           does not flow to the carburetors. Always turn
           the fuel cock knob to this position when the
           engine is not running.
           ON:
           With the fuel cock knob in this position, fuel
           flows to the carburetors. Turn the fuel cock
           knob to this position when starting the engine
           and operating the watercraft.
           RES:
                                                  1 Cooling water pilot outlet
           With the fuel cock knob in this position, the
                                                There is a cooling water pilot outlet on the
           fuel reserve is made available. Turn the fuel
                                                port (left) side of the watercraft. To check for
           cock knob to this position if you run out of

                                                                                 24

| 26 27 28 29 30 31 32 33 34 35 36 |