Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-56
P. 49

    Pre-operation checks

           pouch is securely installed. (See page 27 for  EJU32353
                                                Hull and deck check
           information on the storage pouch.)
                                                Check the hull and deck for damage or other
           EJU41072
           Fire extinguisher container checks   problem.
           Make sure that the fire extinguisher container  EJU32657
                                                Jet intake checks
           is not damaged and is securely held in place.
                                                Make sure that the jet intake is not damaged
           (See page 28 for information on the fire extin-
                                                or clogged with weeds or debris. If the jet in-
           guisher container.)
                                                take is clogged, clean it. (See page 70 for in-
           EJU32494
           Fire extinguisher check              formation on the jet intake.)
           Check that there is a full fire extinguisher on  EJU40703
                                                Hood check
           board.
                                                Make sure that the hood is securely closed.
                                                (See page 26 for information on the hood.)

           To check  the  fire extinguisher, see the  in-
           structions supplied  by the fire extinguisher  EJU40146
           manufacturer. Always keep the fire extin-  Post-launch checks
           guisher in the fire extinguisher container.  Perform the post-launch checks in the pre-
           Always carry a fire extinguisher on board. A  operation checklist while the watercraft is in
           fire extinguisher is not standard  equipment  the water and the engine is running.
           with this watercraft. If you do not have one,  To perform the post-launch checks:
           contact a Yamaha dealer or a fire extinguish-  (1) Launch the watercraft. (See page 45 for
           er dealer to obtain one meeting the proper  information on launching the watercraft.)
           specifications.                      (2) Perform the checks and make sure that
                                                   there are no malfunctioning items or oth-
             Fire extinguisher:                    er problems.
               Classification:
                 B-1
               Capacity:
                 2 lb or more

           EJU40122
           Safety equipment check
           Check that safety equipment meeting the ap-
           plicable regulations is on board.

                                                                                 42

| 44 45 46 47 48 49 50 51 52 53 54 |