Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 33 - LIT-18626-12-56
P. 33

    Equipment operation

           EJU40335                             (2) Turn the latch knob to the “OPEN” posi-
                      Equipment
                                                   tion, and then pull up on the hood latch
           EJU31057
           Hood                                    to unlatch the hood.
           The hood is removable.
           Remove the hood to access the engine com-
           partment.                              1
           To remove the hood:
           (1) Lift the steering pole and support it with
              the lock pin.
                                                       LOCK  OPEN
                                                  2

                                                  1 Hood latch
                                                  2 Hood latch knob
                                                (3) Grasp the hood using the handgrips pro-
                                                   vided at the front and rear of the hood.
                                                   Lift the hood up and to the rear to re-
                                                   move it.
            1 Steering pole

                                                  1 Handgrip
            1 Lock pin

                                                                                 26

| 28 29 30 31 32 33 34 35 36 37 38 |