Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-12-56
P. 65

    Care and storage

           (2) Clean the watercraft. (See page 55 for in-  z Throttle cable (throttle lever end)
              formation on cleaning the watercraft.)  Squeeze the throttle lever and remove the
              Wax the  hull with a non-abrasive wax  seal. Spray Yamaha Lube-Zall into the out-
              such as Yamalube Professional Polish.  er cable. Refit the seal securely.
           EJU40785
           Lubrication
           Use a Yamaha Power Cable Luber and spray
           Yamaha Lube-Zall between the inner and
           outer cables to lubricate  the cables  and
           purge out any dirt and moisture.
           To  keep  moving parts sliding or rotating
           smoothly, lubricate them with water-resistant
           grease.

             Recommended water-resistant grease:
               YAMALUBE MARINE GREASE             1 Seal
                                                z Steering cable ball joint (handlebar end)
           z Throttle cable (carburetor end) and choke
                                                  and steering cable  inner  wire (handlebar
            cable (carburetor end)
                                                  end)
                                                  To access the steering cable ball joint (han-
                                                  dlebar end) and steering cable inner wire
                                                  (handlebar end), remove the steering pole
                                                  cover. (See step 1 in “Adjusting the jet
                                                  thrust nozzle angle” on page 61 for infor-
                                                  mation on removing the steering pole cov-
                                                  er.)

                                                                                 58

| 60 61 62 63 64 65 66 67 68 69 70 |