Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-12-56
P. 72

    Maintenance

           (4) Install the spark plug cap by pushing it  Have a Yamaha dealer replace the fuel filter if
              down  until it is securely installed in its  necessary.
              original position.
           (5) Securely install the  hood in its original
              position.
           EJU41771
           Lubrication points
           Lubricate moving parts with water-resistant
           grease. (See page 58 for information on the
           main lubrication points.)
             Recommended water-resistant grease:
               YAMALUBE MARINE GREASE
                                                  1 Fuel filter
           Intermediate housing                 EJU34442
           Fill the intermediate housing with water-resis-  Adjusting the choke cable
           tant grease through the grease nipple using a  Check that the choke cable is properly ad-
           grease gun.                          justed.
                                                To adjust the choke cable:
             Grease quantity:                   (1) Pull the choke knob out until it stops, and
               Initial 10 hours or 1 month:
                 20.0–22.0 cm³ (0.68–0.74 US oz,   then release the knob. The knob should
                 0.71–0.78 Imp.oz)                 not move.
               Every 100 hours or 12 months:    (2) If the choke  knob moves back  on its
                 3.0–5.0 cm³ (0.10–0.17 US oz,     own, tighten  the choke knob adjusting
                 0.11–0.18 Imp.oz)
                                                   nut slightly. If the knob is difficult to
                                                   move, loosen the adjusting nut slightly.

           EJU34226                               1 Choke knob adjusting nut
           Checking the fuel filter
           Check the fuel filter. The fuel filter should be  EJU34464
                                                Adjusting the carburetor
           replaced if water or dirt is found in the filter.  ECJ00173
                                                 NOTICE
                                                If the carburetor settings are disturbed by
                                                someone who does not have the neces-

           65

| 67 68 69 70 71 72 73 74 75 76 77 |