Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-56
P. 39

    Operation and handling requirements

           (8) Securely install the fuel filler cap by tight-  EJU40022
                                                    Draining the bilge water
              ening it until it clicks.
                                                ECJ01302
           (9) Securely install the  hood in its original  NOTICE
              position.
                                                Do not run the engine at full throttle when
                                                bilge  water remains in the engine com-
                                                partment. The bilge water can splash into
                                                the engine, which  can result  in  severe
                                                damage.

                                                EJU40922
                                                Draining the bilge water on water
                                                A small quantity of bilge water will remain in
                                                the engine compartment even after the bilge
                                                water is drained on water. To completely re-
                                                move the bilge water, remove the watercraft
                                                from the water and wipe  up any  remaining
                                                moisture in the engine compartment with a
                                                dry cloth.
                                                Jet vacuum bilge draining system
                                                While the watercraft is operating, bilge water
                                                in the engine compartment is drawn in by the
                                                vacuum that is generated in the jet pump and
                                                discharged from the watercraft through the
                                                jet thrust nozzle.
                                                To drain the bilge water on water:
                                                Operate the watercraft as straight as possible
                                                and above planing speed for at least 2 min-
                                                utes. NOTICE: Do not run the engine at full
                                                throttle for at least 1 minute after the en-
                                                gine has been restarted. Bilge water in the
                                                engine compartment can splash into the

                                                                                 32

| 34 35 36 37 38 39 40 41 42 43 44 |