Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-12-56
P. 36

    Equipment operation

           (4) Loosen  the fire extinguisher container
              cap and remove it.

            1 Fire extinguisher container cap
           To close the fire extinguisher container:
           (1) Insert the fire extinguisher into the con-
              tainer, and then securely install the fire
              extinguisher container cap by tightening
              it until it stops.
           (2) Lower the container on the hood to its
              storage position  and secure  it with the
              band.
           (3) While  holding the  steering pole, move
              the lock pin to the stowed position, and
              then lower the steering pole.

           29

| 31 32 33 34 35 36 37 38 39 40 41 |