Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - LIT-18626-12-56
P. 40

    Operation and handling requirements

           engine, which can result in severe dam-  EJU33424
                                                          Transporting
           age. [ECJ00554]
                                                EWJ00751
                                                    WARNING
                                                Always turn the fuel cock knob to “OFF”
                                                when transporting the watercraft, other-
                                                wise fuel could leak out into the engine or
                                                engine compartment, which would create
                                                a fire hazard.

                                                When transporting the watercraft on a trailer,
                                                secure the bow  rope hole and stern of  the
                                                watercraft to the  trailer with ropes or tie
                                                downs. Use a rubber shock cord to secure
                                                the steering pole to the watercraft. NOTICE:
                                                Do not secure the steering pole with ropes
                                                or tie downs and do not secure it to the
                                                trailer. Also, do not transport  the water-
                                                craft with the steering pole up. Otherwise,
                                                the steering pole could be damaged. Wrap
                                                the ropes or tie downs with towels or rags

           33

| 35 36 37 38 39 40 41 42 43 44 45 |