Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-56
P. 47

    Pre-operation checks

           whole range, and that the free play is not ex-
                                                  Difference between fully turned posi-
           cessive.                               tions of jet thrust nozzle (distances A
                                                  and B):
                                                    Maximum 5 mm (0.20 in)

                                                EJU32623
                                                Steering pole check
                                                Move the steering pole up and down several
                                                times to make sure that operation is smooth
                                                and unrestricted throughout the whole range,
                                                and that the free play is not excessive. Also,
                                                make sure that the steering pole does not
                                                have any side play.
           Turn the handlebars as far as possible to the
           right and left to make sure that the jet thrust
           nozzle moves as the handlebars are turned,
           and that there is no difference between the
           right and left fully turned positions of the jet
           thrust nozzle.

                                                EJU32595
                                                Throttle lever checks
                                                Operate the throttle lever several times to
                                                make sure that operation is smooth through-
                                                out the whole range. Also, make sure that the
                                                throttle lever returns automatically to its fully
                                                closed (idle) position when released.

                                                                                 40

| 42 43 44 45 46 47 48 49 50 51 52 |