Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-56
P. 66

    Care and storage

           z Steering cable ball joint (jet thrust nozzle  (4) Run the engine at a fast idle.
            end)  and  steering cable inner wire (jet  (5) Quickly spray as much rust inhibitor as
            thrust nozzle end)                     possible through the hole in the silencer
                                                   cover. Use Yamalube Stor-Rite Engine
                                                   Fogging  Oil or an equivalent. Keep
                                                   spraying until the engine stalls (or a max-
                                                   imum of 15 seconds).  WARNING! Do
                                                   not pour or spray gasoline, or any sub-
                                                   stance other  than a rust  inhibitor
                                                   through the hole in the silencer cover.
                                                   Do not spray flammable rust inhibitor
                                                   products on engine surfaces while the
                                                   engine is hot. Otherwise, a fire or ex-
           EJU40935                                plosion could occur. [EWJ00302]
           Rustproofing
                                                (6) Securely install the silencer cap by tight-
           ECJ01361
           NOTICE                                  ening it until it stops. NOTICE: Be sure
                                                   to install the silencer cap securely af-
           Do not run the engine for more than 15
                                                   ter fogging the engine, otherwise wa-
           seconds on land without supplying water,
                                                   ter could enter the engine and cause
           otherwise the engine could overheat.
                                                   damage. [ECJ00153]
           Spray metallic parts of the hull and engine  (7) Securely install the hood in its original
           with a rust inhibitor such as Yamalube Sili-  position.
           cone Protectant & Lubricant.
           To rustproof the internal engine components:
           (1) Remove the hood. (See page 26 for hood
              removal and installation procedures.)
           (2) Loosen the silencer cap and remove it.

            1 Silencer cap
           (3) Make sure that the area around the wa-
              tercraft is clear, and then start the engine
              in a well-ventilated area.

           59

| 61 62 63 64 65 66 67 68 69 70 71 |