Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-12-56
P. 78

    Trouble recovery

           (2) Remove any weeds  or  debris from  (3) Connect the other end of the negative (–)
              around the jet intake, drive shaft, impel-  jumper cable to an unpainted bolt on the
              ler, jet pump housing, and jet thrust noz-  cylinder head.
              zle.
              If debris is difficult to remove, consult a
              Yamaha dealer.
           EJU34642
           Jumping the battery
           If the watercraft battery has run down, the en-
           gine can be started using a 12-volt booster
           battery and jumper cables.
           EJU34654
           Connecting the jumper cables
           EWJ01251
               WARNING                            1 Positive (+) jumper cable
           To avoid  battery  explosion and serious  2 Booster battery
           damage to the electrical system:       3 Negative (–) jumper cable
           z Do not reverse the polarity of the jumper  (4) Start the engine, and then disconnect the
            cables when connecting to the batter-  jumper cables by reversing  the  steps
            ies.                                   above. (See page 22 for information on
           z Do not connect the negative (–) jumper  starting the engine.)
            cable to the negative (–) terminal of the  EJU34676
                                                Replacing the fuse
            watercraft battery.
                                                If the fuse is blown, replace it with the proper
           z Do not touch the positive (+) jumper ca-
                                                fuse.
            ble to the negative (–) jumper cable.
                                                  1                2
           (1) Connect the positive (+) jumper cable to
              the positive (+) battery terminals of both
              batteries.
           (2) Connect one  end of the negative  (–)
              jumper cable to the negative (–) battery
              terminal of the booster battery.

                                                  1 Good fuse
                                                  2 Blown fuse
                                                To replace the fuse:
                                                (1) Remove the hood. (See page 26 for hood
                                                   removal and installation procedures.)
                                                (2) Loosen the cap and remove it.
                                                (3) Pull out the red lead to pull out the fuse
                                                   holder from the electrical box.

           71

| 73 74 75 76 77 78 79 80 81 82 83 |