Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-56
P. 50

    Pre-operation checks

           EJU40553
           Cooling water pilot outlet check
           Make sure that water is discharged from the
           cooling water pilot outlet while the engine is
           running. (See page 24 for information on the
           cooling water pilot outlet.)

           43

| 45 46 47 48 49 50 51 52 53 54 55 |