Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-56
P. 69

    Maintenance

           (3) Remove the steering cable pivot bolt.
                                                TIP:
                                                The outermost  hole in the steering column
                                                cannot be used.

            1 Steering cable pivot bolt
            2 Steering column
           (4) Select the nozzle angle, install the steer-  1 Nozzle angles
              ing cable pivot bolt with the lock washer
              in the desired position (P1 or P2) on the
              steering column, and  then tighten  the
              bolt to the specified torque.

                                                  1 Nozzle angles
                                                  2 Steering cable pivot bolt positions
                                                  Standard steering cable pivot bolt posi-
                                                  tion:
                                                    P2
                                                  Tightening torque:
                                                    Steering cable pivot bolt:
                                                      5 N·m (0.5 kgf·m, 3.7 lb·ft)

                                                (5) Securely connect the steering cable joint
                                                   to the steering cable pivot bolt.
                                                (6) Securely install the steering pole cover
                                                   and two bolts in their original positions.

                                                                                 62

| 64 65 66 67 68 69 70 71 72 73 74 |