Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-56
P. 44

    Pre-operation checks

                    ITEM                         ROUTINE                   PAGE
           POST-LAUNCH CHECKS
                                  Check that water is discharged from the cooling
           Cooling water pilot outlet                                        43
                                  water pilot outlet while the engine is running.
           TIP:
           To ensure safety and reliability, pre-operation checks should be made each time the water-
           craft is used.

           37

| 39 40 41 42 43 44 45 46 47 48 49 |