Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-12-56
P. 79

    Trouble recovery

           (4) Open  the fuse  holder and replace the  z The towline should be long enough so
              fuse with one of the correct amperage.  that the watercraft will not collide with
              WARNING! Do not use fuses of a dif-  the towing boat when slowing down.
              ferent amperage than recommended.
                                                If the watercraft becomes inoperative in the
              Substitution with a fuse that has  an
                                                water, it can be towed to shore.
              improper rating can cause extensive
                                                To tow the watercraft:
              electrical system damage and possi-
                                                Use a towline that is three times the com-
              ble fire. [EWJ00803]
                                                bined length of the towing boat and the wa-
                                                tercraft.
                                                (1) Securely attach the towline to the bow
                                                   rope hole of the watercraft being towed.

            1 Fuse holder
            2 Electrical box
            3 Fuse                                 1
            4 Cap
                                                  1 Bow rope hole
             Fuse amperage:
               Battery fuse:                    (2) Ride the watercraft with  your body
                 10 A                              weight supported on the riding tray. Hold
                                                   on to the handlebars in order to balance
           (5) Insert the fuse holder into the electrical  the watercraft and keep the bow up out
              box.                                 of the water. NOTICE: The bow must be
           (6) Securely install the cap by tightening it  kept up out of the water during tow-
              until it stops.                      ing, otherwise water could flood  the
           (7) Securely install the  hood in its original  engine compartment or water  could
              position.                            flow back into the engine, causing se-
           EJU34705                                vere engine damage. [ECJ01331]
           Towing the watercraft
                                                Tow the watercraft at 8 km/h (5 mph) or less.
           EWJ00812
               WARNING                          NOTICE: Tow the watercraft at 8 km/h (5
                                                mph) or less, otherwise water could flood
           z The  operator of the  towing boat must
                                                the engine  compartment or water could
            keep  speed to a minimum  and avoid
                                                flow back into the engine, causing severe
            traffic or obstacles which could be  a
            hazard to  the operator  on the water-  engine damage. [ECJ01322]
            craft.

                                                                                 72

| 74 75 76 77 78 79 80 81 82 83 84 |