Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-12-56
P. 58

    Operation

           (3) Grip  the handlebars with both hands.  EJU33125
                                                Boarding and starting in deep water
              Place one knee on the riding tray and
                                                EWJ01261
              balance there.                        WARNING
                                                Be sure the operator have practiced
                                                boarding from the water while still close to
                                                shore before riding. A person who  has
                                                made many unsuccessful attempts to get
                                                back on the watercraft may become fa-
                                                tigued and suffer from exposure, increas-
                                                ing the risk of injury and drowning.
                                                (1) Swim to the rear of the watercraft. Attach
                                                   the engine shut-off cord (lanyard) to your
           (4) Look in  all  directions, start the engine,  left wrist, and then attach the clip to the
              and then begin to accelerate.        engine shut-off switch.
           (5) Pull your other knee up onto the riding
              tray as the watercraft speed increases.

                                                (2) Grip the handlebars with  both  hands.
                                                   Pull your body up onto the riding tray and
           (6) Move as far forward as possible without  balance there, using your elbows on the
              interfering with the movement of the han-  gunwales for leverage.
              dlebars. Keep your body perpendicular
              to the water, with your weight forward
              and low.
           TIP:
           The watercraft will become easier to balance
           as the speed increases, because jet thrust
           provides stability as well as directional con-
           trol.

                                                (3) Look  in all directions, start  the  engine,
                                                   and then begin to accelerate.

           51

| 53 54 55 56 57 58 59 60 61 62 63 |